# Simio API Note: MATLAB Custom Steps

Creation: July 2020 (Dan Houck)

Special thanks to Dr. Mohammed Dehghani of NorthEastern U. for the original source code.

Contents

[Simio API Note: MATLAB Custom Steps 1](#_Toc47086820)

[Overview 2](#_Toc47086821)

[Licensing **Error! Bookmark not defined.**](#_Toc47086822)

[Some Background Information on MATLAB 2](#_Toc47086823)

[MATLAB User Step Code 3](#_Toc47086824)

[MATLAB Step Template 3](#_Toc47086825)

[MATLAB Step: MatlabPlaySoundStep 4](#_Toc47086826)

[Simio C# Step Code 4](#_Toc47086827)

[MATLAB Code 6](#_Toc47086828)

[Appendix – Installing the COM Interface to MATLAB 7](#_Toc47086829)

# Overview

This API Note describes how a Simio User-Defined Step can be created to communicate with MATLAB. The original example was derived with permission from the source of Dr. Mohammed Dehghani.

This Note describes some complex programming topics. It assumes that the reader is familiar with C#, MATLAB, and .NET technologies, and that the user has access to a valid MATLAB license.

Before running these examples, the MLApp COM Process from MATLAB must be installed. Please refer to the appendix for instructions on how to do this correctly.

## Some Background Information on MATLAB

What is MATLAB?

From Wikipedia: “MATLAB (matrix laboratory) is a multi-paradigm numerical computing environment and proprietary programming language developed by MathWorks.”

Although originally designed for mathematical operations, it has several add-ons that provide capabilities for machine-learning, robotics, control systems, and other functions.

The company website is here: <https://www.MathWorks.com>

# MATLAB User Step Code

This API Note provides multiple MATLAB steps, which are expected to grow over time. At the core of each is a basic template which involves calling into the MATLAB application and using the MATLAB language. At the time of this writing there are:

1. Play a sound wave file.
2. To be Determined

## MATLAB Step Template

All the MATLAB steps also uses a singleton structure to gain access to the MATLAB application (MLApp). Invoking the MLApp is time consuming, as it is a Windows COM Server, so the singleton pattern allows this to be done only once.

For this to work, the MLApp COM Server must be correctly installed. See the Appendix “Installing the COM Interface to MATLAB” for instructions on how to do this.

The overall organization for a Simio User-Define MATLAB steps is this:

Define the Simio Step definitions so that from within Simio design you can set parameters. For example, the folder and filename properties for a sound file.

Define what happens when the Step is initialized. For example, retrieving the properties that are used when the step is executed, and calling the Matlab context once so that the singleton can store the MATLAB MLApp.

Define what happens each time the Step executes. For example, check the value of a Simio State variable to determine which sound file is to be executed.

By convention, we are going to call the step Matlab<step-function>Step, so our first example step that plays sound files is MatlabPlaySoundStep.

There is a shared MATLAB library called MatlabHelpers that contains code common to all steps, such as logging (tracing).

## MATLAB Step: MatlabPlaySoundStep

The MatlabPlaySoundStep is the “Hello World” step for the MATLAB examples. It is a variation of the example provided by Dr. Mohammed Dehghani.

The Step requires a path to a folder where the MATLAB function files reside, as well as a path to sound files.

When the step is executed, the designated file(s) are played.

This uses the Simio project file ModelTestMatlab1.spfx which is set up to use the following folders:

C:\Test\MatlabFiles – Holds the MATLAB files (e.g. PlaySoundFile.m)

C:\Test\SoundFiles – Holds the sound files (\*.wav and \*.mp3)

### Simio C# Step Code

All the C# code is contained in the MatlabPlaySoundStep.cs file.

The DefineSchema function creates string properties for:

SoundFilePath

MatlabFolderPath

During execution, the CallMatlabPlaySoundFile method is called.

That routine is very simple. After checking for valid arguments, it sets the directory to the MATLAB folder, and then constructs a MATLAB command that is a call to the PlaySoundFile function with the argument being the path to the sound file.

Finally, it looks at the result, which MATLAB formats with returns and “ans =” and parses out the result.

A screenshot of a computer screen

Description automatically generated

### MATLAB Code

The MATLAB function is in a file by the same name within the folder that the C# code pointed to.

The code is exceptionally simple:

A screenshot of a cell phone

Description automatically generated

# Appendix – Installing the COM Interface to MATLAB

A screenshot of a computer

Description automatically generated

Here is the MATLAB link:

<https://www.mathworks.com/help/matlab/matlab_external/register-matlab-as-automation-server.html>

Which should bring you to something that looks like this:

A screenshot of a computer

Description automatically generated

A screenshot of a computer

Description automatically generated

A screenshot of a cell phone

Description automatically generated

To find which version of MATLAB you are communicating with, type:

comserver(‘query’), and the reply should look something like:

A screenshot of a social media post

Description automatically generated

Note: the comserver is available for MATLAB R2020a and later. For previous versions, consult your documentation.

From this command line, you can also test the methods you wish to execute in the Simio Step. For example:

A screenshot of a cell phone

Description automatically generated

You must also register MATLAB as an Automation Server.

This is done by issuing the regmatlabserver command:

A picture containing knife

Description automatically generated

Tips:

***MATLAB commands are case-sensitive!***